redset sets the state of the redstone signal from a specific side of the computer.

ex:
"redset left true" turns on the left redstone output.
"redset right blue false" turns off the blue wire in the bundled cable on the right redstone output.
"redset back 42" sets the wires in the bundled cable on the back redstone output to the binary value 42.
